

**UVC Sterilizer Box**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Item Name** | **Product Picture** | **Speficiations** | **Wireless Charging** | **Exw Price 1000pcs** |
| XD-990 |  | Size：218\*123\*53MM Inner size：180\*100\*22MM UVC wavelength: 253.7mm UVC lamp power：2\*1W Input：DC5VPower：9WN.W.: 340g, G.W.: 440gPacking box： 27x17x6cmCarton size：36pcs/carton,49.5x39.5x30cm G.W.：7.98KG / N.W.：6.97KG | No | US$12.35 |
| Yes | US$13.75 |
| X7 |  | Input:9V/2AOuput:wireless charger 15W/10W/7.5W UVC raidator Power :0.6WUVC wavelength: 275-280nmRecommend Operating temperature :0-40℃ Time for disinfection:≥10s/timeMaterial: ABS+PCProduct size: 170\*91\*41 mmPackage size: 177\*99\*48 mm N.W:174g/G.W: 334gCarton:36x51x21cm, 40pcs/carton,14kgs | Yes | US$16.40 |
| OJD-L02 |  | Input: 5V/2A,9V/2AOutput: 5W 7.5W 10W 15WConversion efficiency:≥78% Charging distance: ≤6mm Dimension outside:53\*114\*196mm, inside:40\*100\*182mm Weight:338gColor:white Material: PC+ABS UVC led: 9pcsWorking frequency:100-205KHZ UV Output:3W 700\*455\*280mmCarton: 700\*455\*280mm, 40pcs/carton,17.7kgs | No | US$18.20 |
| Yes | US$20.70 |
| OJD-L03 |  | Input: 5V/2A,9V/2A Output: 5W 7.5W 10WUVC wavelength: 253.7mm Conversion efficiency:≥78% Charging distance: ≤6mm Dimension: 212.5x120x44mmN.W.: 360gG.W.: 615g Material: PC+ABSPacking: 30pcs/ctn, 49x47x37cm/19.6kgs | Yes | US$23.85 |
| OJD-L05 |  | Input: 5V/2A,9V/2A Output: 5W 7.5W 10WUVC wavelength: 253.7mm Conversion efficiency:≥78% Charging distance: ≤6mm Dimension: 210x120x62mmN.W.: 400gG.W.: 643g Material: PC+ABSPacking: 30pcs/ctn, 49.2x48x34.5cm/20kgs | Yes | US$18.80 |

**Remarks:**

1)Ready to ship in neutral packing 2)Production time: 5-7 days depends on qty 3)Payment term:TT in Advance.

4)Price terms: EXW 5)Certificate: CE,RoHS, FCC